
The latest version of the FT232-R driver is available on FTDI homepage:

<http://www.ftdichip.com/index.html>



**Differences in Driver API**

For most of these operating systems two types of driver are available:

Virtual COM Port (VCP) drivers and direct (D2XX) drivers.

* The VCP driver emulates a standard PC serial port such that the USB device may be communicated with as a standard RS232 device.
* The D2XX driver allows direct access to a USB device via a DLL interface.

To locate the drivers you want to install for a device, select which of the driver types you wish to use ([VCP](http://www.ftdichip.com/Drivers/VCP.htm) or [D2XX](http://www.ftdichip.com/Drivers/D2XX.htm)) and then locate the appropriate operating systems.  With the exception of Windows 98 and Windows ME, all devices are supported in each driver package.

